*---------- DMP4015SK3 Spice Model ----------
.SUBCKT DMP4015SK3 10 20 30 
*     TERMINALS:  D  G  S
M1 1 2 3 3  PMOS  L = 1E-006  W = 1E-006 
RD 10 1 0.00523 
RS 30 3 1E-006 
RG 20 2 7.77 
CGS 2 3 4E-009 
EGD 12 0 1 2 1 
VFB 14 0 0 
FFB 1 2  VFB 1 
CGD 13 14 3.7E-009 
R1 13 0 1 
D1 12 13  DLIM 
DDG 15 14  DCGD 
R2 12 15 1 
D2 15 0  DLIM 
DSD 10 3  DSUB 
.MODEL PMOS PMOS  LEVEL = 3  U0 = 400  VMAX = 1E+006  ETA = 0.02012  
+ TOX = 5E-008  NSUB = 1E+016  KP = 82.85  KAPPA = 0.001  VTO = -2.609 
.MODEL DCGD D  CJO = 1.762E-009  VJ = 0.4937  M = 0.3181 
.MODEL DSUB D  IS = 1.247E-011  N = 1.091  RS = 0.004133  BV = 45  CJO = 1.6E-009  VJ = 0.437  M = 0.3036 
.MODEL DLIM D  IS = 0.0001 
.ENDS
*Diodes DMP4015SK3 Spice Model v1.0 Last Revised 2012/1/13

*---------- DMP4015SSS Spice Model ----------
.SUBCKT DMP4015SSS 10 20 30 
*     TERMINALS:  D  G  S
M1 1 2 3 3  PMOS  L = 1E-006  W = 1E-006 
RD 10 1 0.00523 
RS 30 3 1E-006 
RG 20 2 7.77 
CGS 2 3 4E-009 
EGD 12 0 1 2 1 
VFB 14 0 0 
FFB 1 2  VFB 1 
CGD 13 14 3.7E-009 
R1 13 0 1 
D1 12 13  DLIM 
DDG 15 14  DCGD 
R2 12 15 1 
D2 15 0  DLIM 
DSD 10 3  DSUB 
.MODEL PMOS PMOS  LEVEL = 3  U0 = 400  VMAX = 1E+006  ETA = 0.02012  
+ TOX = 5E-008  NSUB = 1E+016  KP = 82.85  KAPPA = 0.001  VTO = -2.609 
.MODEL DCGD D  CJO = 1.762E-009  VJ = 0.4937  M = 0.3181 
.MODEL DSUB D  IS = 1.247E-011  N = 1.091  RS = 0.004133  BV = 45  CJO = 1.6E-009  VJ = 0.437  M = 0.3036 
.MODEL DLIM D  IS = 0.0001 
.ENDS
*Diodes DMP4015SSS Spice Model v1.0 Last Revised 2012/1/13

*SRC=BSS84;DI_BSS84;MOSFETs P;Enh;50.0V 0.130A 6.00ohms  Diodes Inc. MOSFET
.MODEL DI_BSS84  PMOS( LEVEL=1 VTO=-1.60 KP=4.87m  GAMMA=1.98
+ PHI=.75  LAMBDA=1.25m RD=0.840 RS=0.840
+ IS=65.0f  PB=0.800 MJ=0.460 CBD=46.6p
+ CBS=55.9p  CGSO=50.7n CGDO=42.2n CGBO=69.5n  )
*   -- Assumes default L=100U W=100U --

*SRC=DMP58D0SV;DMP58D0SV_DI;MOSFETs P;Enh;50.0V 0.160A 8.00ohms  Diodes Inc. MOSFET
.MODEL DMP58D0SV_DI  PMOS( LEVEL=1 VTO=-2.10 KP=25.0m  GAMMA=2.60
+ PHI=.75  LAMBDA=133u RD=1.12 RS=1.12
+ IS=80.0f  PB=0.800 MJ=0.460 CBD=12.8p 
+ CBS=15.4p  CGSO=16.8n CGDO=14.0n CGBO=239n  )
*   -- Assumes default L=100U W=100U --

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG_GM
*SIMULATOR=PSPICE
*DATE=10FEB2011
*VERSION=1
*PIN_ORDER D G S
*
.SUBCKT ZXMP6A17N8 1 2 3
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=1.25
M12 22 21 22 20 Npmod1 L=1.4E-6 W=0.95
RG1 21 2 2.8
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.028
RS1 22 23 Rpmod1 0.068
RL1 23 24 7E9
C1 21 22 160E-12
D1 24 23  Dpmod1
LD1 1 24 1.3E-9
LS1 3 23 2.4E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=8.6E-8 NSUB=8E15
+VTO=-2.18 KP=3.5E-5 NFS=3.5E11 KAPPA=0.016 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=8.6E-8 NSUB=6.5E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=2E-12 RS=0.02 IKF=0.1 TRS1=1.5e-3 CJO=85e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=4.6e-3 TC2=8E-6)
.ENDS
*
*$

*SRC=BSS84DW;DI_BSS84DW;MOSFETs P;Enh;50.0V 0.130A 6.00ohms  Diodes Inc. MOSFET- One element of dual
.MODEL DI_BSS84DW  PMOS( LEVEL=1 VTO=-1.60 KP=25.0m  GAMMA=1.98
+ PHI=.75  LAMBDA=108u RD=0.840 RS=0.840
+ IS=65.0f  PB=0.800 MJ=0.460 CBD=43.0p 
+ CBS=51.7p  CGSO=144n CGDO=120n CGBO=186n  )   *   -- Assumes default L=100U W=100U --

*SRC=BSS84W;DI_BSS84W;MOSFETs P;Enh;50.0V 0.130A 6.00ohms  Diodes Inc. MOSFET
.MODEL DI_BSS84W  PMOS( LEVEL=1 VTO=-1.60 KP=25.0m  GAMMA=1.98
+ PHI=.75  LAMBDA=108u RD=0.840 RS=0.840
+ IS=65.0f  PB=0.800 MJ=0.460 CBD=64.2p 
+ CBS=77.1p  CGSO=144n CGDO=120n CGBO=341n  )   *   -- Assumes default L=100U W=100U --

*SRC=DMP57D5UFB;DMP57D5UFB_DI;MOSFETs P;Enh;50.0V 0.200A 6.00ohms  Diodes Inc MOSFET
.MODEL DMP57D5UFB_DI  PMOS( LEVEL=1 VTO=-1.00 KP=0.100  GAMMA=1.24
+ PHI=.75  LAMBDA=250u RD=0.840 RS=0.840
+ IS=100f  PB=0.800 MJ=0.460 CBD=10.9p 
+ CBS=13.1p  CGSO=30.0n CGDO=25.0n CGBO=235n  )
*   -- Assumes default L=100U W=100U --

*SRC=DMP57D5UV;DI_DMP57D5UV;MOSFETs P;Enh;50.0V 0.200A 6.00ohms  Diodes Inc MOSFET
.MODEL DI_DMP57D5UV  PMOS( LEVEL=1 VTO=-1.00 KP=0.100  GAMMA=1.24
+ PHI=.75  LAMBDA=250u RD=0.840 RS=0.840
+ IS=100f  PB=0.800 MJ=0.460 CBD=10.9p 
+ CBS=13.1p  CGSO=30.0n CGDO=25.0n CGBO=235n  )
*   -- Assumes default L=100U W=100U --

*
*Zetex ZXM64P035L3 Spice Model v1.0 Last Revised 23/5/02
*
.SUBCKT ZXM64P035L3 3 4 5
*----connections----D G S
*
M1 6 2 8 8 MOSMOD
M2 6 2 8 8 MOSMODS
RG 4 2 9
RIN 2 8 200E6
RD 3 6 RDSMOD 0.02
RS 8 5 RDSMOD 0.015 
RL 3 5 35E6
C1 2 8 810E-12
C3 15 14 1050E-12 
C4 16 8 1150E-12
D1 3 5 DMOD1
D2 3 17 DMOD2
S1 2 15 13 14 SMOD1a
S2 13 15 13 14 SMOD1b
S3 16 13 8 13 SMOD2a
S4 16 2 8 13 SMOD2b
Egs1 2 17 2 8 1
Egs2 13 8 2 8 1
Eds1 14 8 3 8 1
.MODEL MOSMOD PMOS VTO=-2.4 IS=1E-15 KP=8 CBD=512E-12 PB=1 LAMBDA=4.9E-3
.MODEL MOSMODS PMOS VTO=-2 IS=1E-15 KP=0.1 PB=1
.MODEL DMOD1 D IS=6E-13 RS=0.02 N=1.01 TT=1e-8
.MODEL DMOD2 D CJO=430e-12 IS=1e-30 N=10
.MODEL SMOD1a VSWITCH RON=1e-2 ROFF=1e4  VON=-1.75 VOFF=2.75
.MODEL SMOD1b VSWITCH RON=1e-2 ROFF=1e4  VON=2.75 VOFF=-1.75
.MODEL SMOD2a VSWITCH RON=1e-2 ROFF=1e4  VON=-1.5 VOFF=-3.5
.MODEL SMOD2b VSWITCH RON=1e-2 ROFF=1e4  VON=-3.5 VOFF=-1.5
.MODEL RDSMOD RES (TC1=3E-3 TC2=1.5E-5)
.ENDS ZXM64P035L3
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP6A13G Spice Model v2.0 Last Revised 15/02/05
*
.SUBCKT zxmp6a13G 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.2E-6 W=0.39
M2 5 2 5 6 Nmod L=1.4E-6 W=0.195
RG 4 2 3
RIN 2 5 1E9
RD 3 6 Rdmod 0.25
RL 3 5 3E9
C1 2 5 25E-12
C2 3 4 15E-12
D1 3 5  Dbodymod
LD 3 30 1E-9
LG 4 40 2.3E-9
LS 5 50 2.3E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=5.5E-8 NSUB=1e16
+VTO=-1.5 KP=6e-6 RS=0.005 NFS=12e11 KAPPA=0.01 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=5.5E-8 NSUB=1E16
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=1e-11 RS=0.05 IKF=0.001966 XTI=-1 TRS1=1.2e-3
+CJO=3.514e-11  BV=66)
.MODEL Rdmod RES (TC1=5e-3 TC2=1e-5)
.ENDS zxmp6a13G
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=25/02/2009
*VERSION=1
*PIN_ORDER         D G S
*
.SUBCKT ZXMP6A17E6 1 2 3
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=1.25
M12 22 21 22 20 Npmod1 L=1.4E-6 W=0.95
RG1 21 27 2.8
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.028
RS1 22 23 Rpmod1 0.068
RL1 23 24 7E9
C1 21 22 160E-12
D1 24 23  Dpmod1
LD1 1 24 0.3E-9
LG1 2 27 1.2E-9
LS1 3 23 1.2E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=8.6E-8 NSUB=8E15
+VTO=-2.18 KP=3.5E-5 NFS=3.5E11 KAPPA=0.016 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=8.6E-8 NSUB=6.5E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=2E-12 RS=0.02 IKF=0.1 TRS1=1.5e-3 CJO=85e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=4.6e-3 TC2=8E-6)
.ENDS
*
*$

*
*Zetex BS250P Spice Model v1.0 Last Revised 19/3/03
*
.SUBCKT BS250P 3 4 5
*                D G S
M1 3 2 5 5 MBS250
RG 4 2 160
RL 3 5 1.2E8
C1 2 5 47E-12
C2 3 2 10E-12 
D1 3 5 DBS250
*
.MODEL MBS250 PMOS VTO=-3.193 RS=2.041 RD=0.697 IS=1E-15 KP=0.277
+CBD=105E-12 PB=1 LAMBDA=1.2E-2
.MODEL DBS250 D IS=2E-13 RS=0.309
.ENDS BS250P
*
*$

*SRC=BSS84V;DI_BSS84V;MOSFETs P;Enh;50.0V 0.130A 6.00ohms  Diodes Inc. MOSFET
.MODEL DI_BSS84V  PMOS( LEVEL=1 VTO=-1.60 KP=4.87m  GAMMA=1.98
+ PHI=.75  LAMBDA=1.25m RD=0.840 RS=0.840
+ IS=65.0f  PB=0.800 MJ=0.460 CBD=46.6p 
+ CBS=55.9p  CGSO=50.7n CGDO=42.2n CGBO=69.5n  )
*   -- Assumes default L=100U W=100U --

*
*Zetex ZVP3306F Spice Model v1.1 Last Revised 3/5/00
*
.SUBCKT ZVP3306F 3 4 5
*                D G S
M1 3 2 5 5 P3306M
RG 4 2 252
RL 3 5 1.2E8
C1 2 5 28E-12
C2 3 2 3E-12 
D1 3 5 P3306D
*
.MODEL P3306M PMOS VTO=-2.875 RS=5.227 RD=7.524 IS=1E-15 KP=.145
+CBD=35E-12 PB=1 LAMBDA=6.67E-3
.MODEL P3306D D IS=5E-12 RS=.768
.ENDS ZVP3306F
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP6A13F Spice Model v2.0 Last Revised 15/02/05
*
.SUBCKT zxmp6a13F 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.2E-6 W=0.39
M2 5 2 5 6 Nmod L=1.4E-6 W=0.195
RG 4 2 3
RIN 2 5 1E9
RD 3 6 Rdmod 0.25
RL 3 5 3E9
C1 2 5 25E-12
C2 3 4 15E-12
D1 3 5  Dbodymod
LD 3 30 0.5E-9
LG 4 40 1.0E-9
LS 5 50 1.0E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=5.5E-8 NSUB=1e16
+VTO=-1.5 KP=6e-6 RS=0.005 NFS=12e11 KAPPA=0.01 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=5.5E-8 NSUB=1E16
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=1e-11 RS=0.05 IKF=0.001966 XTI=-1 TRS1=1.2e-3
+CJO=3.514e-11  BV=66)
.MODEL Rdmod RES (TC1=5e-3 TC2=1e-5)
.ENDS zxmp6a13F
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=27/10/2008
*VERSION=2
*PIN_ORDER         D G S
*
.SUBCKT ZXMP6A16K 1 2 3
*Dev1 P-channel
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=2.148
M12 22 21 22 20 Npmod1 L=1.4E-6 W=1.579
RG1 21 27 1.9
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.04
RS1 22 23 1E-6
RL1 23 24 7E9
D1 24 23  Dpmod1
LD1 1 24 1.3E-9
LG1 2 27 2.4E-9
LS1 3 23 2.4E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=10.7E-8 NSUB=6.6E15
+VTO=-2.24 KP=1.4E-5 RS=.03 NFS=1E11 KAPPA=.005 UO=650 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=10.7E-8 NSUB=6.45E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=5E-12 RS=.02 IKF=0.02 TRS1=1.5e-3 CJO=380e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=6.1e-3 TC2=2.8E-5)
.ENDS
*
*$

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=25/02/2009
*VERSION=1
*PIN_ORDER         D G S
*
.SUBCKT ZXMP6A17K 1 2 3
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=1.25
M12 22 21 22 20 Npmod1 L=1.4E-6 W=0.95
RG1 21 27 2.8
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.028
RS1 22 23 Rpmod1 0.068
RL1 23 24 7E9
C1 21 22 160E-12
D1 24 23  Dpmod1
LD1 1 24 1.3E-9
LG1 2 27 2.4E-9
LS1 3 23 2.4E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=8.6E-8 NSUB=8E15
+VTO=-2.18 KP=3.5E-5 NFS=3.5E11 KAPPA=0.016 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=8.6E-8 NSUB=6.5E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=2E-12 RS=0.02 IKF=0.1 TRS1=1.5e-3 CJO=85e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=4.6e-3 TC2=8E-6)
.ENDS ZXMP6A17K
*
*$

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=04/02/2009
*VERSION=3
*PIN_ORDER         Sp1, Gp1, Sp2, Gp2, Dp2, Dp2, Dp1, Dp1
*
.SUBCKT ZXMP6A18DN8 1 2 3 4 5 6 7 8
*Dev1 P-channel
M11 20 21 22 22 Ppmod1 L=1.2E-6 W=2.64
M12 22 21 22 20 Npmod1 L=1.4E-6 W=1.5
RG1 27 21 1.3
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.03
RS1 22 23 1e-6
RL1 23 24 3E9
C11 21 22 500E-12
C12 20 21 15E-12
D1 24 23  Dpmod1
LD1 24 25 1.5E-9
RP11 7 25 1E-6
RP12 8 25 1E-6
LG1 2 27 1.2E-9
LS1 1 23 1.2E-9
*Dev2 P-channel
M21 60 61 62 62 Ppmod1 L=1.2E-6 W=2.64
M22 62 61 62 60 Npmod1 L=1.4E-6 W=1.5
RG2 67 61 1.3
RIN2 61 62 1E9
RD2 60 64 Rpmod1 0.03
RS2 62 63 1e-6
RL2 63 64 3E9
C21 61 62 500E-12
C22 60 61 15E-12
D2 64 63  Dpmod1
LD2 64 65 1.5E-9
RP21 5 65 1E-6
RP22 6 65 1E-6
LG2 4 67 1.2E-9
LS2 3 63 1.2E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=5.5E-8 NSUB=.5E17 VTO=-1.83
+KP=1.9E-5 RS=.035 NFS=2E11 KAPPA=0.06 UO=650 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=5.5E-8 NSUB=1E16
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=1.6E-12 RS=.022 IKF=1 TRS1=1.5e-3
+CJO=65e-12  BV=66)
.MODEL Rpmod1 RES (TC1=10e-3 TC2=8E-6)
.ENDS
*
*$

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=25/02/2009
*VERSION=3
*PIN_ORDER         D G S
*
.SUBCKT ZXMP6A18K 1 2 3
M11 20 21 22 22 Ppmod1 L=1.2E-6 W=2.64
M12 22 21 22 20 Npmod1 L=1.4E-6 W=1.5
RG1 27 21 1.3
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.03
RS1 22 23 1E-6
RL1 23 24 3E9
C11 21 22 500E-12
C12 20 21 15E-12
D1 24 23  Dpmod1
LD1 1 24 1.3E-9
LG1 2 27 2.4E-9
LS1 3 23 2.4E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=5.5E-8 NSUB=.5E17 VTO=-1.83
+KP=1.9E-5 RS=0.035 NFS=2E11 KAPPA=0.06 UO=650 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=5.5E-8 NSUB=1E16
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=1.6E-12 RS=.022 IKF=1 TRS1=1.5E-3
+CJO=65E-12  BV=66)
.MODEL Rpmod1 RES (TC1=10e-3 TC2=8E-6)
.ENDS
*
*$

*
*ZETEX ZXMP7A17G Spice Model v1.0 Last Revised 14/3/2007
*
.SUBCKT ZXMP7A17G 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.35E-6 W=1.082
M2 5 2 5 6 Nmod L=1.8E-6 W=0.6
RG 4 2 1.9
RIN 2 5 1E9
RD 3 6 Rdmod 0.07
RL 3 5 7E9
D1 3 5  Dbodymod
LD 3 30 1.0E-9
LG 4 40 2.3E-9
LS 5 50 2.3E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=5.5E-8 NSUB=50E15
+VTO=-1.77 KP=2.5E-5 RS=.05 NFS=2E11 KAPPA=.002 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=5.5E-8 NSUB=5.2E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=5E-12 RS=.02 IKF=0.02 TRS1=1.5e-3 CJO=380e-12 
+M=0.43 VJ=0.41 TT=2.2e-8  BV=77)
.MODEL Rdmod RES (TC1=9e-3 TC2=1.5E-5)
.ENDS
*
*$
*                (c)  2007 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP2106A Spice Model v1.1 Last Revised 3/5/00
*
.SUBCKT ZVP2106A 3 4 5
*                D G S
M1 3 2 5 5 MP2106
RG 4 2 160
RL 3 5 1.2E8
C1 2 5 47E-12
C2 3 2 10E-12 
D1 3 5 DP2106
*
.MODEL MP2106 PMOS VTO=-3.193 RS=2.041 RD=0.697 IS=1E-15 KP=0.277
+CBD=105E-12 PB=1 LAMBDA=1.2E-2
.MODEL DP2106 D IS=2E-13 RS=0.309
.ENDS ZVP2106A
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP2106G Spice Model v1.1 Last Revised 3/5/00
*
.SUBCKT ZVP2106G 3 4 5
*                D G S
M1 3 2 5 5 MP2106
RG 4 2 160
RL 3 5 1.2E8
C1 2 5 47E-12
C2 3 2 10E-12 
D1 3 5 DP2106
*
.MODEL MP2106 PMOS VTO=-3.193 RS=2.041 RD=0.697 IS=1E-15 KP=0.277
+CBD=105E-12 PB=1 LAMBDA=1.2E-2
.MODEL DP2106 D IS=2E-13 RS=0.309
.ENDS ZVP2106G
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP3306A Spice Model v1.1 Last Revised 3/5/00
*
.SUBCKT ZVP3306A 3 4 5
*                D G S
M1 3 2 5 5 P3306M
RG 4 2 252
RL 3 5 1.2E8
C1 2 5 28E-12
C2 3 2 3E-12
D1 3 5 P3306D
*
.MODEL P3306M PMOS VTO=-2.875 RS=5.227 RD=7.524 IS=1E-15 KP=.145
+CBD=35E-12 PB=1 LAMBDA=6.67E-3
.MODEL P3306D D IS=5E-12 RS=.768
.ENDS ZVP3306A
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP4105A Spice Model v1.0 Last revision 31/3/05
*              
.SUBCKT ZVP4105A 3 4 5
* NODES: DRAIN GATE SOURCE
M1 3 2 5 5 MOD1
RG 4 2 167
RL 3 5 50E6
C1 2 5 26P
C2 3 2 4P 
D1 3 5 DIODE1
*
.MODEL MOD1 PMOS VTO=-1.709 RS=3.091 RD=0.979 IS=1E-15 KP=0.146
+CBD=12P PB=1
.MODEL DIODE1 D IS=1.072E-13 RS=0.527 N=1.077
.ENDS ZVP4105A
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP4A16G Spice Model v1.0 Last Revised 22/6/06
*
.SUBCKT ZXMP4A16G 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.2E-6 W=1.67 
M2 5 2 5 6 Nmod L=1.4E-6 W=0.96
RG 4 2 2
RIN 2 5 1E9
RD 3 6 Rdmod 0.018
RL 3 5 3E9
C1 2 5 40E-12
C2 3 4 25E-12
D1 3 5  Dbodymod
LD 3 30 1E-9
LG 4 40 2.3E-9
LS 5 50 2.3E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=5.5E-8 NSUB=4E16
+VTO=-1.8 KP=1.6E-5 RS=.022 NFS=2E11 KAPPA=0.06 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=5.5E-8 NSUB=2E16 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=5E-12 RS=.018 IKF=0.1 TRS1=1.5e-3
+CJO=450e-12 TT=2.2e-8  BV=44)
.MODEL Rdmod RES (TC1=8e-3 TC2=1.5E-5)
.ENDS   ZXMP4A16G
*
*$
*
*                (c)  2006 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=04/02/2009
*VERSION=3
*PIN_ORDER         Sp1, Gp1, Sp2, Gp2, Dp2, Dp2, Dp1, Dp1
*
.SUBCKT ZXMP6A17DN8 1 2 3 4 5 6 7 8
*Dev1 P-channel
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=1.25
M12 22 21 22 20 Npmod1 L=1.4E-6 W=0.95
RG1 21 27 2.8
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.028
RS1 22 23 Rpmod1 0.068
RL1 23 24 7E9
C1 21 22 160E-12
D1 24 23  Dpmod1
LD1 24 25 1.5E-9
RP11 7 25 1E-6
RP12 8 25 1E-6
LG1 2 27 1.2E-9
LS1 1 23 1.2E-9
*Dev2 P-channel
M21 60 61 62 62 Ppmod1 L=1.4E-6 W=1.25
M22 62 61 62 60 Npmod1 L=1.4E-6 W=0.95
RG2 61 67 2.8
RIN2 61 62 1E9
RD2 60 64 Rpmod1 0.028
RS2 62 63 Rpmod1 0.068
RL2 63 64 7E9
C2 61 62 160E-12
D2 64 63  Dpmod1
LD2 64 65 1.5E-9
RP21 5 65 1E-6
RP22 6 65 1E-6
LG2 4 67 1.2E-9
LS2 3 63 1.2E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=8.6E-8 NSUB=8E15
+VTO=-2.18 KP=3.5E-5 NFS=3.5E11 KAPPA=0.016 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=8.6E-8 NSUB=6.5E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=2E-12 RS=0.02 IKF=0.1 TRS1=1.5e-3 CJO=85e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=4.6e-3 TC2=8E-6)
.ENDS
*
*$

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=25/02/2009
*VERSION=1
*PIN_ORDER         D G S
*
.SUBCKT ZXMP6A17G 1 2 3
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=1.25
M12 22 21 22 20 Npmod1 L=1.4E-6 W=0.95
RG1 21 27 2.8
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.028
RS1 22 23 Rpmod1 0.068
RL1 23 24 7E9
C1 21 22 160E-12
D1 24 23  Dpmod1
LD1 1 24 1.0E-9
LG1 2 27 2.3E-9
LS1 3 23 2.3E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=8.6E-8 NSUB=8E15
+VTO=-2.18 KP=3.5E-5 NFS=3.5E11 KAPPA=0.016 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=8.6E-8 NSUB=6.5E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=2E-12 RS=0.02 IKF=0.1 TRS1=1.5e-3 CJO=85e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=4.6e-3 TC2=8E-6)
.ENDS
*
*$

*
*ZETEX ZXMP7A17K Spice Model v1.0 Last Revised 14/3/2007
*
.SUBCKT ZXMP7A17K 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.35E-6 W=1.082
M2 5 2 5 6 Nmod L=1.8E-6 W=0.6
RG 4 2 1.9
RIN 2 5 1E9
RD 3 6 Rdmod 0.07
RL 3 5 7E9
D1 3 5  Dbodymod
LD 3 30 1.3E-9
LG 4 40 2.4E-9
LS 5 50 2.4E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=5.5E-8 NSUB=50E15
+VTO=-1.77 KP=2.5E-5 RS=.05 NFS=2E11 KAPPA=.002 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=5.5E-8 NSUB=5.2E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=5E-12 RS=.02 IKF=0.02 TRS1=1.5e-3 CJO=380e-12 
+M=0.43 VJ=0.41 TT=2.2e-8  BV=77)
.MODEL Rdmod RES (TC1=9e-3 TC2=1.5E-5)
.ENDS
*
*$
*                (c)  2007 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP4A16K Spice Model v1.0 Last Revised 09/10/06
*
.SUBCKT ZXMP4A16K 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.2E-6 W=1.67 
M2 5 2 5 6 Nmod L=1.4E-6 W=0.96
RG 4 2 2
RIN 2 5 1E9
RD 3 6 Rdmod 0.018
RL 3 5 3E9
C1 2 5 40E-12
C2 3 4 25E-12
D1 3 5  Dbodymod
LD 3 30 1.3E-9
LG 4 40 2.4E-9
LS 5 50 2.4E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=5.5E-8 NSUB=4E16
+VTO=-1.8 KP=1.6E-5 RS=.022 NFS=2E11 KAPPA=0.06 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=5.5E-8 NSUB=2E16 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=5E-12 RS=.018 IKF=0.1 TRS1=1.5e-3
+CJO=450e-12 TT=2.2e-8  BV=44)
.MODEL Rdmod RES (TC1=8e-3 TC2=1.5E-5)
.ENDS   ZXMP4A16K
*
*$
*
*                (c)  2006 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG
*SIMULATOR=PSPICE
*DATE=04/02/2009
*VERSION=3
*PIN_ORDER         D G S
*
.SUBCKT ZXMP6A16DN8 1 2 3 4 5 6 7 8
*Dev1 P-channel
M11 20 21 22 22 Ppmod1 L=1.4E-6 W=2.148
M12 22 21 22 20 Npmod1 L=1.4E-6 W=1.579
RG1 21 27 1.9
RIN1 21 22 1E9
RD1 20 24 Rpmod1 0.04
RS1 22 23 1E-6
RL1 23 24 7E9
D1 24 23  Dpmod1
LD1 24 25 1.5E-9
RP11 7 25 1E-6
RP12 8 25 1E-6
LG1 2 27 1.2E-9
LS1 1 23 1.2E-9
*Dev2 P-channel
M21 60 61 62 62 Ppmod1 L=1.4E-6 W=2.148
M22 62 61 62 60 Npmod1 L=1.4E-6 W=1.579
RG2 61 67 1.9
RIN2 61 62 1E9
RD2 60 64 Rpmod1 0.04
RS2 62 63 1E-6
RL2 63 64 7E9
D2 64 63  Dpmod1
LD2 64 65 1.5E-9
RP21 5 65 1E-6
RP22 6 65 1E-6
LG2 4 67 1.2E-9
LS2 3 63 1.2E-9
.MODEL Ppmod1 PMOS (LEVEL=3 TOX=10.7E-8 NSUB=6.6E15
+VTO=-2.24 KP=1.4E-5 RS=.03 NFS=1E11 KAPPA=.005 UO=650 IS=1E-15 N=10)
.MODEL Npmod1 NMOS (LEVEL=3 TOX=10.7E-8 NSUB=6.45E15 
+TPG=-1 IS=1E-15 N=10)
.MODEL Dpmod1 D (IS=5E-12 RS=.02 IKF=0.02 TRS1=1.5e-3 CJO=380e-12 
+M=0.43 VJ=0.41 TT=3.2e-8  BV=66)
.MODEL Rpmod1 RES (TC1=6.1e-3 TC2=2.8E-5)
.ENDS
*
*$