*
*ZETEX ZMR500 Spice Model v1.0 Last revision 31/01/07
*
.SUBCKT ZMR500 1 2 3 
* Connections  IN_GND_OUT
Q1 12 5 6 Qmod1
R1 4 2 Rmod1 1
R2 6 7 0.04
R4 10 2 15E3
R5 6 8 1E6
R6 5 6 1E6
D1 1 11 Dmod1
D2 11 12 Dmod1
R8 7 2 Rmod3 100E3
C4 8 10 130E-12
I1 2 4 5.001
G1 5 7 8 4 1
G2 2 4 1 2 5E-4
VS 3 7 0
F1 2 4 VS 0.5
.MODEL Qmod1 NPN (RC=10 RB=10 RE=10 CJC=2p CJE=5p)
.MODEL Dmod1 D (IS=0.8E-15)
.MODEL Rmod1 RES (TC1=-3.9E-5 TC2=-6.1E-7)
.MODEL Rmod3 RES (TC1=-5E-4 TC2=0E-7)
.ENDS ZMR500
*
*$
*
*                (c)  2007 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL