*
*ZETEX ZVP4525E6  Spice model v1.0  Last revision 6/01/2005
*
.SUBCKT  ZVP4525E6 3 4 5
*---connections---D-G-S
M1 6 20 8 8 MOSMOD1
M2 6 20 8 8 MOSMOD2
RG 4 2 7
RIN 2 8 200E6
RD 3 6 RMOD1 11
RS 8 5 RMOD1 0.5
RB 3 7 RMOD1 0.2
RL 3 5 250E6
C1 2 8 80E-12
C2 2 3  12E-12
C3 15 14 175E-12
C4 16 8 175E-12
D1 7 5 DMOD1
S1 2 15 14 13 SMOD1a
S2 13 15 14 13 SMOD1b
S3 16 13 13 8 SMOD2a
S4 16 2 13 8 SMOD2b
Egs2 13 8 2 8 1
Eds1 14 8 3 8 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 RMOD2 1
.MODEL MOSMOD1 PMOS VTO=-1.5 IS=1E-15 KP=0.15
.MODEL MOSMOD2 PMOS VTO=-.9 IS=1E-15 KP=0.0015
.MODEL DMOD1 D IS=4.14E-13 N=1.0078 CJO=100E-12 BV=260
.MODEL SMOD1a VSWITCH RON=.01 ROFF=1e3  VON=1.7 VOFF=-2.75
.MODEL SMOD1b VSWITCH RON=.01 ROFF=1e3  VON=-2.75 VOFF=1.7
.MODEL SMOD2a VSWITCH RON=.01 ROFF=1e3  VON=1.5 VOFF=3.5
.MODEL SMOD2b VSWITCH RON=.01 ROFF=1e3  VON=3.5 VOFF=1.5
.MODEL RMOD1 RES (TC1=8e-3 TC2=1.5e-5)
.MODEL RMOD2 RES (TC1=-1.9e-3 TC2=1e-6)
.ENDS
*
*$
*
*                  (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc ("Zetex").  They  are  supplied  
*   free of charge by Zetex for the purpose of research and design 
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*ZETEX ZVP4525Z  Spice model v1.0  Last revision 6/01/2005
*
.SUBCKT  ZVP4525Z 3 4 5
*---connections---D-G-S
M1 6 20 8 8 MOSMOD1
M2 6 20 8 8 MOSMOD2
RG 4 2 7
RIN 2 8 200E6
RD 3 6 RMOD1 11
RS 8 5 RMOD1 0.5
RB 3 7 RMOD1 0.2
RL 3 5 250E6
C1 2 8 80E-12
C2 2 3  12E-12
C3 15 14 175E-12
C4 16 8 175E-12
D1 7 5 DMOD1
S1 2 15 14 13 SMOD1a
S2 13 15 14 13 SMOD1b
S3 16 13 13 8 SMOD2a
S4 16 2 13 8 SMOD2b
Egs2 13 8 2 8 1
Eds1 14 8 3 8 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 RMOD2 1
.MODEL MOSMOD1 PMOS VTO=-1.5 IS=1E-15 KP=0.15
.MODEL MOSMOD2 PMOS VTO=-.9 IS=1E-15 KP=0.0015
.MODEL DMOD1 D IS=4.14E-13 N=1.0078 CJO=100E-12 BV=260
.MODEL SMOD1a VSWITCH RON=.01 ROFF=1e3  VON=1.7 VOFF=-2.75
.MODEL SMOD1b VSWITCH RON=.01 ROFF=1e3  VON=-2.75 VOFF=1.7
.MODEL SMOD2a VSWITCH RON=.01 ROFF=1e3  VON=1.5 VOFF=3.5
.MODEL SMOD2b VSWITCH RON=.01 ROFF=1e3  VON=3.5 VOFF=1.5
.MODEL RMOD1 RES (TC1=8e-3 TC2=1.5e-5)
.MODEL RMOD2 RES (TC1=-1.9e-3 TC2=1e-6)
.ENDS
*
*$
*
*                  (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc ("Zetex").  They  are  supplied  
*   free of charge by Zetex for the purpose of research and design 
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP10A13F Spice Model v1.0 Last Revised 15/11/07
*
.SUBCKT ZXMP10A13F 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.2E-6 W=0.33
M2 5 2 5 6 Nmod L=1.4E-6 W=0.19
RG 4 2 10
RIN 2 5 1E9
RD 3 6 Rdmod 0.55
RL 3 5 3E9
C1 2 5 50E-12
C2 3 4 1E-12
D1 3 5  Dbodymod
LD 3 30 0.5E-9
LG 4 40 1.0E-9
LS 5 50 1.0E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=11E-8 NSUB=1e16
+VTO=-3.4 KP=6e-6 RS=0.05 NFS=14E11 KAPPA=0.05 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=11E-8 NSUB=3.6E15
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=1.8e-13 RS=0.07 CJO=25E-12 TT=55E-9 BV=105)
.MODEL Rdmod RES (TC1=6.8e-3 TC2=1e-5)
.ENDS ZXMP10A13F
*
*$
*
*                (c)  2007 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP10A16K Spice Model v1.0 Last Revised 21/11/07
*
.SUBCKT ZXMP10A16K 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.35E-6 W=1.68
M2 5 2 5 6 Nmod L=1.4E-6 W=1.15
RG 4 2 4.7
RIN 2 5 1E9
RD 3 6 Rdmod 0.1
RL 3 5 3E9
C1 2 5 50E-12
C2 3 4 1E-12
D1 3 5  Dbodymod
LD 3 30 1.3E-9
LG 4 40 2.4E-9
LS 5 50 2.4E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=11E-8 NSUB=0.3e16
+VTO=-3.2 KP=5.2e-6 RS=0.035 NFS=7.5E11 KAPPA=0.05 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=11E-8 NSUB=3.6E15
+TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=1e-12 RS=0.027 CJO=125E-12 TT=66E-9 BV=105)
.MODEL Rdmod RES (TC1=9e-3 TC2=1e-5)
.ENDS ZXMP10A16K
*
*$
*
*                (c)  2007 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP10A17E6 Spice model v1.0 Last revision 06/08/08
*
.SUBCKT ZXMP10A17E6 30 40 50
*                                  D G S
M1 6 2 5 5 Pmod L=1.35E-6 W=1.082
M2 5 2 5 6 Nmod L=1.8E-6 W=0.6
RG 4 2 4.2
RIN 2 5 1E9
RD 3 6 Rdmod 0.185
RL 3 5 7E9
D1 3 5  Dbodymod
LD 3 30 0.3E-9
LG 4 40 1.9E-9
LS 5 50 1.9E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=9.5E-8 NSUB=5E15
+ VTO=-3.7 KP=0.6E-5 RS=0.05 NFS=0.8E12 KAPPA=0.03 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=9.5E-8 NSUB=2.5E15 TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=7.5E-13 RS=.06 TRS1=1.5e-3 CJO=120e-12 M=0.43 VJ=0.41 TT=5.2e-8  BV=110)
.MODEL Rdmod RES (TC1=7.8e-3 TC2=1.4E-5)
.ENDS   ZXMP10A17E6
*
*$
*
*                (c)  2008 Diodes Incorporated
*
*   The copyright in these models  and  the designs embodied belong
*   to Diodes Incorporated (" Diodes ").  They  are  supplied
*   free of charge by Diodes for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Diodes Incorporated, its distributors
*   or agents.
*
*   Diodes Incorporated, 1566 N. Dallas Parkway, Suite 850, Dallas, TX 75248, USA

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG_GM
*SIMULATOR=PSPICE
*DATE=17SEP2010
*VERSION=1
*------connections------- D, G, S
.SUBCKT ZXMP10A17G 30 40 50
M1 6 2 5 5 Pmod L=1.35E-6 W=1.082
M2 5 2 5 6 Nmod L=1.8E-6 W=0.6
RG 4 2 4.2
RIN 2 5 1E9
RD 3 6 Rdmod 0.185
RL 3 5 7E9
D1 3 5  Dbodymod
LD 3 30 0.3E-9
LG 4 40 1.9E-9
LS 5 50 1.9E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=9.5E-8 NSUB=5E15
+ VTO=-3.7 KP=0.6E-5 RS=0.05 NFS=0.8E12 KAPPA=0.03 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=9.5E-8 NSUB=2.5E15 TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=7.5E-13 RS=.06 TRS1=1.5e-3 CJO=120e-12 M=0.43 VJ=0.41
+ TT=5.2e-8  BV=110)
.MODEL Rdmod RES (TC1=7.8e-3 TC2=1.4E-5)
.ENDS   ZXMP10A17G
*
*$

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG_GM
*SIMULATOR=PSPICE
*DATE=17SEP2010
*VERSION=1
*------connections------- D, G, S
.SUBCKT ZXMP10A17K 30 40 50
M1 6 2 5 5 Pmod L=1.35E-6 W=1.082
M2 5 2 5 6 Nmod L=1.8E-6 W=0.6
RG 4 2 4.2
RIN 2 5 1E9
RD 3 6 Rdmod 0.185
RL 3 5 7E9
D1 3 5  Dbodymod
LD 3 30 0.3E-9
LG 4 40 1.9E-9
LS 5 50 1.9E-9
.MODEL Pmod PMOS (LEVEL=3 TOX=9.5E-8 NSUB=5E15
+ VTO=-3.7 KP=0.6E-5 RS=0.05 NFS=0.8E12 KAPPA=0.03 UO=650 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=9.5E-8 NSUB=2.5E15 TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=7.5E-13 RS=.06 TRS1=1.5e-3 CJO=120e-12 M=0.43 VJ=0.41
+ TT=5.2e-8  BV=110)
.MODEL Rdmod RES (TC1=7.8e-3 TC2=1.4E-5)
.ENDS   ZXMP10A17K
*
*$

*
*Zetex ZVP4424A Spice Model v2.0 Last Revised 17/07/2008
*
.SUBCKT ZVP4424A 3 4 5
*------connections-------D-G-S
*
M1 6 2 8 8 P4424AM
M2 6 2 8 8 P4424AMS
RG 4 2 27
RD 3 6 5.5
RS 8 5 0.6 
RL 3 5 240E6
D1 3 5 P4424AD
Egs2 13 8 2 8 1
Eds1 14 8 6 8 1
C1 2 8 125E-12
C2 2 3  15E-12
C3 15 14 210E-12 
C4 16 8 220E-12
S1 2 15 14 13 SMOD1
S2 13 15 14 13 SMOD2
S3 16 13 13 8 SMOD3
S4 16 2 13 8 SMOD4
.MODEL SMOD1 VSWITCH RON=.001 ROFF=100 VON=-1 VOFF=-2
.MODEL SMOD2 VSWITCH RON=.001 ROFF=100 VON=-2 VOFF=-1
.MODEL SMOD3 VSWITCH RON=.001 ROFF=100  VON=2.5 VOFF=3.5
.MODEL SMOD4 VSWITCH RON=.001 ROFF=100  VON=3.5 VOFF=2.5
.MODEL P4424AM PMOS VTO=-1.4 IS=1E-15 KP=0.26 CBD=65.3E-12 PB=1
.MODEL P4424AMS PMOS VTO=-1.04 IS=1E-15 KP=0.0026 CBD=270E-12 PB=1
.MODEL P4424AD D IS=9.36E-13 RS=.196 N=1.045
.ENDS ZVP4424A
*
*$
*
*                (c)  2008 Diodes Incorporated
*
*   The copyright in these models  and  the designs embodied belong
*   to Diodes Incorporated (" Diodes ").  They  are  supplied
*   free of charge by Diodes for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Diodes Incorporated, its distributors
*   or agents.
*
*   Diodes Incorporated, 1566 N. Dallas Parkway, Suite 850, Dallas, TX 75248, USA

*
*Zetex ZVP4424G Spice Model v2.0 Last Revised 17/07/2008
*
.SUBCKT ZVP4424G 3 4 5
*------connections-------D-G-S
*
M1 6 2 8 8 P4424AM
M2 6 2 8 8 P4424AMS
RG 4 2 27
RD 3 6 5.5
RS 8 5 0.6 
RL 3 5 240E6
D1 3 5 P4424AD
Egs2 13 8 2 8 1
Eds1 14 8 6 8 1
C1 2 8 125E-12
C2 2 3  15E-12
C3 15 14 210E-12 
C4 16 8 220E-12
S1 2 15 14 13 SMOD1
S2 13 15 14 13 SMOD2
S3 16 13 13 8 SMOD3
S4 16 2 13 8 SMOD4
.MODEL SMOD1 VSWITCH RON=.001 ROFF=100 VON=-1 VOFF=-2
.MODEL SMOD2 VSWITCH RON=.001 ROFF=100 VON=-2 VOFF=-1
.MODEL SMOD3 VSWITCH RON=.001 ROFF=100  VON=2.5 VOFF=3.5
.MODEL SMOD4 VSWITCH RON=.001 ROFF=100  VON=3.5 VOFF=2.5
.MODEL P4424AM PMOS VTO=-1.4 IS=1E-15 KP=0.26 CBD=65.3E-12 PB=1
.MODEL P4424AMS PMOS VTO=-1.04 IS=1E-15 KP=0.0026 CBD=270E-12 PB=1
.MODEL P4424AD D IS=9.36E-13 RS=.196 N=1.045
.ENDS ZVP4424G
*
*$
*
*                (c)  2008 Diodes Incorporated
*
*   The copyright in these models  and  the designs embodied belong
*   to Diodes Incorporated (" Diodes ").  They  are  supplied
*   free of charge by Diodes for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Diodes Incorporated, its distributors
*   or agents.
*
*   Diodes Incorporated, 1566 N. Dallas Parkway, Suite 850, Dallas, TX 75248, USA

*
*ZETEX ZVP4525G  Spice model v1.0  Last revision 6/01/2005
*
.SUBCKT  ZVP4525G 3 4 5
*---connections---D-G-S
M1 6 20 8 8 MOSMOD1
M2 6 20 8 8 MOSMOD2
RG 4 2 7
RIN 2 8 200E6
RD 3 6 RMOD1 11
RS 8 5 RMOD1 0.5
RB 3 7 RMOD1 0.2
RL 3 5 250E6
C1 2 8 80E-12
C2 2 3  12E-12
C3 15 14 175E-12
C4 16 8 175E-12
D1 7 5 DMOD1
S1 2 15 14 13 SMOD1a
S2 13 15 14 13 SMOD1b
S3 16 13 13 8 SMOD2a
S4 16 2 13 8 SMOD2b
Egs2 13 8 2 8 1
Eds1 14 8 3 8 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 RMOD2 1
.MODEL MOSMOD1 PMOS VTO=-1.5 IS=1E-15 KP=0.15
.MODEL MOSMOD2 PMOS VTO=-.9 IS=1E-15 KP=0.0015
.MODEL DMOD1 D IS=4.14E-13 N=1.0078 CJO=100E-12 BV=260
.MODEL SMOD1a VSWITCH RON=.01 ROFF=1e3  VON=1.7 VOFF=-2.75
.MODEL SMOD1b VSWITCH RON=.01 ROFF=1e3  VON=-2.75 VOFF=1.7
.MODEL SMOD2a VSWITCH RON=.01 ROFF=1e3  VON=1.5 VOFF=3.5
.MODEL SMOD2b VSWITCH RON=.01 ROFF=1e3  VON=3.5 VOFF=1.5
.MODEL RMOD1 RES (TC1=8e-3 TC2=1.5e-5)
.MODEL RMOD2 RES (TC1=-1.9e-3 TC2=1e-6)
.ENDS
*
*$
*
*                  (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc ("Zetex").  They  are  supplied  
*   free of charge by Zetex for the purpose of research and design 
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZXMP10A18G Spice Model v2.0 Last Revised 08/04/08
*
.SUBCKT ZXMP10A18G 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.3E-6 W=2.64
M2 5 2 5 6 Nmod L=1.4E-6 W=2.0
RG 4 2 4.5
RIN 2 5 1E9
RD 3 6 Rdmod 0.085
RL 3 5 3E9
C1 2 5 50E-12
C2 3 4 1E-12
D1 3 5 Dbodymod
LD 3 30 1.0E-9
LG 4 40 2.3E-9
LS 5 50 2.3E-9
*
.MODEL Pmod PMOS (LEVEL=3 TOX=11E-8 NSUB=1.2e16 VTO=-3.5 KP=6.1e-6
+ RS=0.02 NFS=6E11 KAPPA=0.05 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=11E-8 NSUB=3.6E15
+ TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=1.3e-12 RS=0.025 CJO=25E-12 TT=65E-9 BV=105)
.MODEL Rdmod RES (TC1=7.5e-3 TC2=1.4e-5)
.ENDS ZXMP10A18G
*
*$
*
*                (c)  2008 Diodes Incorporated
*
*   The copyright in these models  and  the designs embodied belong
*   to Diodes Incorporated (" Diodes ").  They  are  supplied
*   free of charge by Diodes for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Diodes Incorporated, its distributors
*   or agents.
*
*   Diodes Incorporated, 1566 N. Dallas Parkway, Suite 850, Dallas, TX 75248, USA

*
*Zetex ZXMP10A18K Spice Model v2.0 Last Revised 08/04/08
*
.SUBCKT ZXMP10A18K 30 40 50
*                D G S
M1 6 2 5 5 Pmod L=1.3E-6 W=2.64
M2 5 2 5 6 Nmod L=1.4E-6 W=2.0
RG 4 2 4.5
RIN 2 5 1E9
RD 3 6 Rdmod 0.085
RL 3 5 3E9
C1 2 5 50E-12
C2 3 4 1E-12
D1 3 5 Dbodymod
LD 3 30 1.3E-9
LG 4 40 2.4E-9
LS 5 50 2.4E-9
*
.MODEL Pmod PMOS (LEVEL=3 TOX=11E-8 NSUB=1.2e16 VTO=-3.5 KP=6.1e-6
+ RS=0.02 NFS=6E11 KAPPA=0.05 IS=1E-15 N=10)
.MODEL Nmod NMOS (LEVEL=3 TOX=11E-8 NSUB=3.6E15
+ TPG=-1 IS=1E-15 N=10)
.MODEL Dbodymod D (IS=1.3e-12 RS=0.025 CJO=25E-12 TT=65E-9 BV=105)
.MODEL Rdmod RES (TC1=7.5e-3 TC2=1.4e-5)
.ENDS ZXMP10A18K
*
*$
*
*                (c)  2008 Diodes Incorporated
*
*   The copyright in these models  and  the designs embodied belong
*   to Diodes Incorporated (" Diodes ").  They  are  supplied
*   free of charge by Diodes for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Diodes Incorporated, its distributors
*   or agents.
*
*   Diodes Incorporated, 1566 N. Dallas Parkway, Suite 850, Dallas, TX 75248, USA

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG_GM
*SIMULATOR=PSPICE
*DATE=10FEB2011
*VERSION=1
*PIN_ORDER D G S
*
.SUBCKT ZXMP2120E5 3 4 5
M1 13 20 5 5 Pmod1
RG 4 2 100
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 22
C1 2 5 55E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+ CBD=60E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=2 BV=220
.MODEL Dmod2 D CJO=70e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=4.5e-3 TC2=4E-5)
.MODEL Rmod2 RES (TC1=-2.5e-3 TC2=3e-6)
.ENDS
*
*$

*
*Zetex ZVP1320F Spice Model v1.0 Last Revised 13/06/02
*
.SUBCKT ZVP1320F 3 4 5
*                D G S
M1 6 2 8 8 MOSMOD
M2 6 2 8 8 MOSMODS
RG 4 2 56
RIN 2 8 200E6
RD 3 6 RDSMOD 71
RS 8 5 RDSMOD 6.6 
RL 3 5 200E6
C1 2 8 42E-12
D1 3 5 DMOD1
D2 3 17 DMOD2
Egs1 2 17 2 8 1
.MODEL MOSMOD PMOS VTO=-2.56 IS=1E-15 KP=.059 CBD=15E-12 PB=1 LAMBDA=4.9E-3
.MODEL MOSMODS PMOS VTO=-2.2 IS=1E-15 KP=0.002 PB=1
.MODEL DMOD1 D IS=2E-13 RS=0.12 N=1.01 IKF=3e-3
.MODEL DMOD2 D CJO=18e-12 IS=1e-30 N=10
.MODEL RDSMOD RES (TC1=8E-3 TC2=3E-5)
.ENDS ZVP1320F
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP3310F Spice Model v1.1 Last Revised 22/7/04
*
.SUBCKT ZVP3310F 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 50
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 5
C1 2 5 55E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.1 RS=2 IS=1E-15 KP=0.2
+CBD=35E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=1
.MODEL Dmod2 D CJO=20e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=9e-3 TC2=4.2E-5)
.MODEL Rmod2 RES (TC1=-2e-3 TC2=3e-6)
.ENDS ZVP3310F
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP4424Z Spice Model v1.0 Last Revised 17/07/2008
*
.SUBCKT ZVP4424Z 3 4 5
*------connections-------D-G-S
*
M1 6 2 8 8 P4424AM
M2 6 2 8 8 P4424AMS
RG 4 2 27
RD 3 6 5.5
RS 8 5 0.6 
RL 3 5 240E6
D1 3 5 P4424AD
Egs2 13 8 2 8 1
Eds1 14 8 6 8 1
C1 2 8 125E-12
C2 2 3  15E-12
C3 15 14 210E-12 
C4 16 8 220E-12
S1 2 15 14 13 SMOD1
S2 13 15 14 13 SMOD2
S3 16 13 13 8 SMOD3
S4 16 2 13 8 SMOD4
.MODEL SMOD1 VSWITCH RON=.001 ROFF=100 VON=-1 VOFF=-2
.MODEL SMOD2 VSWITCH RON=.001 ROFF=100 VON=-2 VOFF=-1
.MODEL SMOD3 VSWITCH RON=.001 ROFF=100  VON=2.5 VOFF=3.5
.MODEL SMOD4 VSWITCH RON=.001 ROFF=100  VON=3.5 VOFF=2.5
.MODEL P4424AM PMOS VTO=-1.4 IS=1E-15 KP=0.26 CBD=65.3E-12 PB=1
.MODEL P4424AMS PMOS VTO=-1.04 IS=1E-15 KP=0.0026 CBD=270E-12 PB=1
.MODEL P4424AD D IS=9.36E-13 RS=.196 N=1.045
.ENDS ZVP4424Z
*
*$
*
*                (c)  2008 Diodes Incorporated
*
*   The copyright in these models  and  the designs embodied belong
*   to Diodes Incorporated (" Diodes ").  They  are  supplied
*   free of charge by Diodes for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Diodes Incorporated, its distributors
*   or agents.
*
*   Diodes Incorporated, 1566 N. Dallas Parkway, Suite 850, Dallas, TX 75248, USA

*
*DIODES_INC_SPICE_MODEL
*ORIGIN=DZSL_DPG_GM
*SIMULATOR=PSPICE
*DATE=10FEB2011
*VERSION=1
*PIN_ORDER D G S
*
.SUBCKT ZXMP2120G4 3 4 5
M1 13 20 5 5 Pmod1
RG 4 2 100
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 22
C1 2 5 55E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+ CBD=60E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=2 BV=220
.MODEL Dmod2 D CJO=70e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=4.5e-3 TC2=4E-5)
.MODEL Rmod2 RES (TC1=-2.5e-3 TC2=3e-6)
.ENDS
*
*$

*
*Zetex ZVP0545A Spice Model v1.0 Last Revised 4/8/2004
*              
*
.SUBCKT ZVP0545A 3 4 5
*                D G S
M1 6 20 8 8 MOSMOD
M2 6 20 8 8 MOSMODS
RG 4 2 85
RIN 2 8 200E6
RD 3 6 RMOD1 71
RS 8 5 RMOD1 6.6 
RL 3 5 200E6
C1 2 8 110E-12
D1 3 5 DMOD1
D2 3 17 DMOD2
Egs1 2 17 2 8 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 RMOD2 1
.MODEL MOSMOD PMOS VTO=-2.56 IS=1E-15 KP=.059 CBD=15E-12 PB=1 LAMBDA=4.9E-3
.MODEL MOSMODS PMOS VTO=-2.2 IS=1E-15 KP=0.002 PB=1
.MODEL DMOD1 D IS=2E-13 RS=10 N=1.01 IKF=3e-3
.MODEL DMOD2 D CJO=18e-12 IS=1e-30 N=10
.MODEL RMOD1 RES (TC1=8E-3 TC2=1.7E-5)
.MODEL RMOD2 RES (TC1=-2.5e-3 TC2=3.3e-6)
.ENDS
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP0545G Spice Model v1.2 Last Revised 20/05/2004
*              
*
.SUBCKT ZVP0545G 3 4 5
*                D G S
M1 6 20 8 8 MOSMOD
M2 6 20 8 8 MOSMODS
RG 4 2 85
RIN 2 8 200E6
RD 3 6 RMOD1 71
RS 8 5 RMOD1 6.6 
RL 3 5 200E6
C1 2 8 110E-12
D1 3 5 DMOD1
D2 3 17 DMOD2
Egs1 2 17 2 8 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 RMOD2 1
.MODEL MOSMOD PMOS VTO=-2.56 IS=1E-15 KP=.059 CBD=15E-12 PB=1 LAMBDA=4.9E-3
.MODEL MOSMODS PMOS VTO=-2.2 IS=1E-15 KP=0.002 PB=1
.MODEL DMOD1 D IS=2E-13 RS=10 N=1.01 IKF=3e-3
.MODEL DMOD2 D CJO=18e-12 IS=1e-30 N=10
.MODEL RMOD1 RES (TC1=8E-3 TC2=1.7E-5)
.MODEL RMOD2 RES (TC1=-2.5e-3 TC2=3.3e-6)
.ENDS
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP2110A Spice Model v1.0 Last Revised 23/7/04
*
.SUBCKT ZVP2110A 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 65
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 2.5
C1 2 5 140E-12
**C2 3 2 15E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+CBD=105E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=1
.MODEL Dmod2 D CJO=60e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=8e-3 TC2=4.2E-5)
.MODEL Rmod2 RES (TC1=-2e-3 TC2=3e-6)
.ENDS ZVP2110A
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*Zetex ZVP2110G Spice Model v1.0 Last Revised 22/7/04
*
.SUBCKT ZVP2110G 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 65
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 2.5
C1 2 5 140E-12
**C2 3 2 15E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+CBD=105E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=1
.MODEL Dmod2 D CJO=60e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=8e-3 TC2=4.2E-5)
.MODEL Rmod2 RES (TC1=-2e-3 TC2=3e-6)
.ENDS ZVP2110G
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*ZETEX ZVP2120A Spice Model v1.0 Last Revised 10/8/05
*
.SUBCKT ZVP2120A 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 100
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 22
C1 2 5 55E-12
**C2 3 2 15E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+CBD=60E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=2 BV=220
.MODEL Dmod2 D CJO=70e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=4.5e-3 TC2=4E-5)
.MODEL Rmod2 RES (TC1=-2.5e-3 TC2=3e-6)
.ENDS ZVP2120A
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL
.

*
*ZETEX ZVP2120G Spice Model v1.0 Last Revised 10/8/05
*
.SUBCKT ZVP2120G 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 100
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 22
C1 2 5 55E-12
**C2 3 2 15E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+CBD=60E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=2 BV=220
.MODEL Dmod2 D CJO=70e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=4.5e-3 TC2=4E-5)
.MODEL Rmod2 RES (TC1=-2.5e-3 TC2=3e-6)
.ENDS ZVP2120G
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL
.

*
*Zetex ZVP3310A Spice Model v1.0 Last Revised 23/7/04
*
.SUBCKT ZVP3310A 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 50
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 5
C1 2 5 55E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.1 RS=2 IS=1E-15 KP=0.2
+CBD=35E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=1
.MODEL Dmod2 D CJO=20e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=9e-3 TC2=4.2E-5)
.MODEL Rmod2 RES (TC1=-2e-3 TC2=3e-6)
.ENDS ZVP3310A
*
*$
*
*                (c)  2005 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL

*
*ZETEX ZXMP2120FF Spice Model v1.0 Last Revised 09/02/07
*
.SUBCKT ZXMP2120FF 3 4 5
*                D G S
M1 13 20 5 5 Pmod1
RG 4 2 100
RIN 2 5 1E9
RL 3 5 1.2E8
RD 3 13 Rmod1 22
C1 2 5 55E-12
**C2 3 2 15E-12
D1 3 5 Dmod1
D2 3 17 Dmod2
Egs1 2 17 2 5 1
Egt1 2 20 5 21 1
Vgt1 5 22 1
Igt1 5 21 1
Rgt 21 22 Rmod2 1
.MODEL Pmod1 PMOS VTO=-2.8 RS=2 IS=1E-15 KP=0.17
+CBD=60E-12 PB=1 LAMBDA=6E-3
.MODEL Dmod1 D IS=5E-12 RS=2 BV=220
.MODEL Dmod2 D CJO=70e-12 IS=1e-30 N=10
.MODEL Rmod1 RES (TC1=4.5e-3 TC2=4E-5)
.MODEL Rmod2 RES (TC1=-2.5e-3 TC2=3e-6)
.ENDS ZXMP2120FF
*
*$
*
*                (c)  2007 Zetex Semiconductors plc
*
*   The copyright in these models  and  the designs embodied belong
*   to Zetex Semiconductors plc (" Zetex ").  They  are  supplied
*   free of charge by Zetex for the purpose of research and design
*   and may be used or copied intact  (including this notice)  for
*   that purpose only.  All other rights are reserved. The models
*   are believed accurate but  no condition  or warranty  as to their
*   merchantability or fitness for purpose is given and no liability
*   in respect of any use is accepted by Zetex PLC, its distributors
*   or agents.
*
*   Zetex Semiconductors plc, Zetex Technology Park, Chadderton,
*   Oldham, United Kingdom, OL9 9LL
.